**User Manual of GPS Demo Module for RSP;SAIL**

* Press the power button on top side of the device for atleast 2 seconds to power on . The device will vibrate for power-on confirmation.
* Press the power button for atleast 3 seconds and then release to power off the device. As long as the button is not released, the device will not power off.
* The device has low battery indicator RED led below the power button when battery percentage goes below 20%.
* The device will automatically power off if its battery percentage goes below 8%.
* The device has charging indicator WHITE led at the same position of low battery indication below power button.
* It is recommended to charge the devices only after turning them off.
* Once the devices will attached to any metal, it will vibrate once each time as confirmation of proper attachment to user.
* It is recommended to turn off the device when not in use.

It will enhance battery life.

* User can track the devices through laptop,desktop or mobile by loging into the URL 45.64.237.125:3301 with default user ID and password.
* After log in select the devices from All Payloader dropdown like , DSS\_Demo\_1 or DSS\_Demo\_2 or DSS\_Demo\_4.
* User can track device’s status remotely like, device moving speed,available battery percentage or metal attachment status by clicking on the location symbol for each devices on live map view.